----setTabletComPort() options----
For Topaz USB-connected ("-HSB") pads, use:
"HID1"

For Topaz 9-pin serial pads (under Windows) use:
"COMX"
(where X is the port in question, for instance: COM1)

For Linux and 9-pin serial pads, for instance:
"/dev/ttyS0"




----setTabletModel() options----
1. TL(BK)460 and TL(BK)462:
"SignatureGemLCD1X5"


2. TS261:
"SignatureGem1X5"


3. TS751:
"SignatureGem4X5"


4. TL(BK)755-B and TL(BK)750-B:
"SignatureGemLCD4X3New"

*For TLBK755-BHSB and TLBK750-BHSB:
"SignatureGemLCD4X3New"
and
setTabletBaudRate(38400)

*For TLBK755SE-BHSB TLBK750SE-BHSB use:
"SignatureGemLCD4X3New"
and
setTabletBaudRate(115200)


5. TL(BK)766-B:
"SignatureGemLCD4X5"

*For TLBK766-BHSB, use:
"SignatureGemLCD4X5"
and
setTabletBaudRate(38400)

*For TLBK766SE-BHSB, use:
"SignatureGemLCD4X5"
and
setTabletBaudRate(115200)


6. TC912:
"ClipGem"


7. TC916:
"ClipGemLGL"


8. TLBK57GC
"SigGemColor57"
and
setTabletBaudRate(115200)

9. TLBK43LC
"SigLiteColor43"
and
setTabletBaudRate(115200)