Overview | Package | Class | Tree | Deprecated | Index | Help
| Topaz Systems, Inc. SigPlus v2.41
PREV NEXT | FRAMES NO FRAMES

A C E G H I K L N S

## A

autoKeyData(string)-Method in class com.topaz.SigPlus
  Adds data to the auto key generation function.
autoKeyFinish()-Method in class com.topaz.SigPlus
  Completes the auto key generation function.
autoKeyStart()-Method in class com.topaz.SigPlus
  Initializes the automatic key generation function.

## C

clearTablet()-Method in class com.topaz.SigPlus
  Clears the signature from the object.

## E

exportSigFile()-Method in class com.topaz.SigPlus
  Writes a signature file in the Topaz image-free raw tablet vector file (.sig extension).

## G

getAnnotation()-Method in class com.topaz.SigPlus
  Returns current ASCII line character.
getDisplayAnnotation()-Method in class com.topaz.SigPlus
  Returns whether or not the Annotation is being displayed.
getDisplayAnnotationSize()-Method in class com.topaz.SigPlus
  Returns Annotation size in pixels.
getDisplayAnnotationX()-Method in class com.topaz.SigPlus
  Returns the X position in pixels of the start of the Annotation string in the signature box.
getDisplayAnnotationY()-Method in class com.topaz.SigPlus
  Returns the Y position in pixels of the start of the Annotation string in the signature box.
getDisplayJustifyMode()-Method in class com.topaz.SigPlus
  Returns the justification mode, how the image is set in the signature box.
getDisplayJustifyX()-Method in class com.topaz.SigPlus
  Returns current justify X buffer in pixels.
getDisplayJustifyY()-Method in class com.topaz.SigPlus
  Returns current justify Y buffer in pixels.
getDisplayPenWidth()-Method in class com.topaz.SigPlus
  Returns current pen width setting.
getDisplayRotation()-Method in class com.topaz.SigPlus
  Returns the current display rotation setting.
getDisplayTimeStamp()-Method in class com.topaz.SigPlus
  Returns whether or not the Time Stamp is being displayed.
getDisplayTimeStampSize()-Method in class com.topaz.SigPlus
  Returns the size in pixels of the Time Stamp.
getDisplayTimeStampX()-Method in class com.topaz.SigPlus
  Returns current X position in pixels of the start of the Time Stamp in the signature box.
getDisplayTimeStampY()-Method in class com.topaz.SigPlus
  Returns current Y position in pixels of the start of the Time Stamp in the signature box.
getDisplayTransparentMode()-Method in class com.topaz.SigPlus
  Returns whether or not the tablet is in Transparent Mode.
getEncryptionMode()-Method in class com.topaz.SigPlus
  Returns the current encryption mode for capturing signatures.
getImageAnnotation()-Method in class com.topaz.SigPlus
  Returns whether or not the Annotation is being displayed as it apllies to a Java buffered image.
getImageAnnotationSize()-Method in class com.topaz.SigPlus
  Returns the size in pixels of the Annotation as it applies to a Java buffered image.
getImageAnnotationX()-Method in class com.topaz.SigPlus
  Returns the X position in pixels of the Annotation as it applies to a Java buffered image.
getImageAnnotationY()-Method in class com.topaz.SigPlus
  Returns the Y position in pixels of the Annotation as it applies to a Java buffered image.
getImageJustifyMode()-Method in class com.topaz.SigPlus
  Returns the justification mode as it applies to a Java buffered image.
getImageJustifyX()-Method in class com.topaz.SigPlus
  Returns the current justify X buffer as it apllies to a Java buffered image.
getImageJustifyY()-Method in class com.topaz.SigPlus
  Returns the current justify Y buffera s it applies to a Java buffered image.
getImagePenWidth()-Method in class com.topaz.SigPlus
  Returns current pen width setting as it applies to a Java buffered image.
getImageRotation()-Method in class com.topaz.SigPlus
  Returns the display rotation setting as it applies to a Java buffered image.
getImageTimeStamp()-Method in class com.topaz.SigPlus
  Returns whether ot not the Time Stamp is being displayed as it applies to a Java buffered image.
getImageTimeStampSize()-Method in class com.topaz.SigPlus
  Returns the size in pixels of the start of the Time Stamp as it applies to a Java buffered image.
getImageTimeStampX()-Method in class com.topaz.SigPlus
  Returns the X position in pixels of the start of the Time Stamp as it applies to a Java buffered image.
getImageTimeStampY()-Method in class com.topaz.SigPlus
  Returns the Y position of the start of the Time Stamp as it applies to a Java buffered image.
getImageTransparentMode()-Method in class com.topaz.SigPlus
  Returns whether or not the tablet is in transparent mode as it applies to a Java buffered image.
getImageXSize()-Method in class com.topaz.SigPlus
  Returns width in pixels of Image as it applies to a Java buffered image.
getImageYSize()-Method in class com.topaz.SigPlus
  Returns height in pixels of Image as it applies to a Java buffered image.
getKeyString()-Method in class com.topaz.SigPlus
  Provides the encryption key from the control in ASCII compatible format.
getLCDCaptureMode()-Method in class com.topaz.SigPlus
  Returns current LCD mode for the tablet.
getNumberOfStrokes()-Method in class com.topaz.SigPlus
  Returns total number of strokes in the current signature and can detect the presence of a signature.
getNumPointsForStroke()-Method in class com.topaz.SigPlus
  Returns total number of points in a specified stroke.
getPointXValue (short, short)-Method in class com.topaz.SigPlus
  Returns the X coordinate value for the specified point in Logical Tablet Coordinates.
getPointYValue(short, short)-Method in class com.topaz.SigPlus
  Returns the Y coordinate value for the specified point in Logical Tablet Coordinates.
getSigCompressionMode()-Method in class com.topaz.SigPlus
  Returns the current compression mode for signatures.
getSigPlusVersion()-Method in class com.topaz.SigPlus
  Returns the current version of the SigPlus JAR file as a string.
getSigReceipt()-Method in class com.topaz.SigPlus
  Returns a 32 bit receipt similar to the key receipt.
getSigReceiptAscii(short, short)-Method in class com.topaz.SigPlus
  Same as `getKeyReceiptAscii`, but for Sig Reciept.
getSigString()-Method in class com.topaz.SigPlus
  Removes the signature out of the bean.
getTabletBaudRate()-Method in class com.topaz.SigPlus
  Returns the baud rate for the tablet.
getTabletClippingMode()-Method in class com.topaz.SigPlus
  Returns whether Tablet Clipping Mode is active ot not.
getTabletComPort()-Method in class com.topaz.SigPlus
  Returns the current COM port assignment.
getTabletComTest()-Method in class com.topaz.SigPlus
  Returns if tablet is connected.
getTabletFilterPoints()-Method in class com.topaz.SigPlus
  Returns the Tablet Filter Points.
getTabletFormat()-Method in class com.topaz.SigPlus
  Returns the current tablet format.
getTabletInvisible()-Method in class com.topaz.SigPlus
  Returns whether or not Tablet Invisible is active.
getTabletLCDType()-Method in class com.topaz.SigPlus
  Returns current LCD type of tablet.
getTabletLCDXSize()-Method in class com.topaz.SigPlus
  Returns current LCD width in pixels.
getTabletLCDXStart()-Method in class com.topaz.SigPlus
  Returns current X pos in Logical Tablet Coordinates of left most pixel.
getTabletLCDXStop()-Method in class com.topaz.SigPlus
  Returns current X pos in Logical Tablet Coordinates of right most pixel.
getTabletLCDYSize()-Method in class com.topaz.SigPlus
  Returns current LCD height in pixels.
getTabletLCDYStart()-Method in class com.topaz.SigPlus
  Returns current Y pos in Logical Tablet Coordinates of the top most pixel.
getTabletLCDYStop()-Method in class com.topaz.SigPlus
  Returns the current Y pos in Logical Tablet Coordinates of the bottom most pixel.
getTabletLogicalXSize()-Method in class com.topaz.SigPlus
  Returns the range of horizontal values to be used in representing signatures in Logical Tablet Coordinates.
getTabletLogicalYSize()-Method in class com.topaz.SigPlus
  Returns the range of vertical values to be used in representing signatures in Logical Tablet Coordinates.
getTabletModel()-Method in class com.topaz.SigPlus
  Returns the current model of the signature tablet.
getTabletResolution()-Method in class com.topaz.SigPlus
  Returns the resolution settings for the signature tablet.
getTabletRotation()-Method in class com.topaz.SigPlus
  Returns the orientation for the display of tablet data.
getTabletState()-Method in class com.topaz.SigPlus
  Returns the state of the tablet open or closed.
getTabletTimingAdvance()-Method in class com.topaz.SigPlus
  Returns the Tablet Timing Advance.
getTabletXStart()-Method in class com.topaz.SigPlus
  Returns the current X position of the top left corner of the signature box in Logical Tablet Coordinates.
getTabletXStop()-Method in class com.topaz.SigPlus
  Returns the current X position of the bottom right corner of the signature box in Logical Tablet Coordinates.
getTabletYStart()-Method in class com.topaz.SigPlus
  Returns the current Y position of the top left corner of the signature box in Logical Tablet Coordinates.
getTabletYStop()-Method in class com.topaz.SigPlus
  Returns the current Y position of the bottom right corner of the signature box in Logical Tablet Coordinates.
getTimeStamp()-Method in class com.topaz.SigPlus
  Returns the Time Stamp string for the signature.
getXExtent()-Method in class com.topaz.SigPlus
  Returns the exact width in pixels of the current signature.
getYExtent()-Method in class com.topaz.SigPlus
  Returns the exact height in pixels of the current signature.

## H

handleKeyPadData (SigPlusEvent0 evt)-method in interface com.topaz.SigPlus.SigEventDataHandler
  Fires when KeyPadHotSpot hit
handleNewTabletData (SigPlusEvent0 evt)-method in interface com.topaz.SigPlus.SigEventDataHandler
  Not Currently Implemented
handleTabletTimerEvent (SigPlusEvent0 evt)-method in interface com.topaz.SigPlus.SigEventDataHandler
  NotCurrentlyImplemented

## I

importSigFile(string)-Method in class com.topaz.SigPlus
  Clears the current signature, reads in a signature file in the Topaz vector file format, and displays it.

## K

keyPadAddHotSpot(int, int, int, int, int, int)-Method in class com.topaz.SigPlus
  Defines in software the location of a tablet HotSpot in Logical Tablet Coordinates.
keyPadClearHotSpotList()-Method in class com.topaz.SigPlus
  Clears the control's internal list of HotSpots.
keyPadClearSigWindow(int)-Method in class com.topaz.SigPlus
  Erases data either inside or outside of the sig window based on the value on `int inside`.
keyPadQueryHotSpot(int)-Method in class com.topaz.SigPlus
  Queries the data points currently in the control against the Logical Tablet Coordinates mapped by KeyCode.
keyPadSetSigWindow(int, int, int, int, int)-Method in class com.topaz.SigPlus
  Sets a window in Logical Tablet space that restricts the operations of some functions to the specified window.

## L

lcdRefresh(int, int, int, int, int)-Method in class com.topaz.SigPlus
  Sends refresh command to the tablet
lcdSetWindow(int, int, int, int)-Method in class com.topaz.SigPlus
  Sets the tablet so that the LCD display wil be showing ink only in a restricted area when data is input from a pen in LCDCaptureMode.
lcdWriteImage(int, int, int, int, int, int, int, Image)-Method in class com.topaz.SigPlus
  Writes windows bitmap data to the LCD Display at the location specified by combination of dest, xPos, Ypos.

## N

numberOfTabletPoints()-Method in class com.topaz.SigPlus
  Returns the total number of points in the current signature and can be used to detect if a signature is present or not.

## S

setAnnotation(string)-Method in class com.topaz.SigPlus
  Sets the ASCII line character.
setDisplayAnnotation(string)-Method in class com.topaz.SigPlus
  Sets the bean to display the Annotation string.
setDisplayAnnotationSize(int)-Method in class com.topaz.SigPlus
  Sets the Y size in pixels of the Annotation string.
setDisplayAnnotationX(int)-Method in class com.topaz.SigPlus
  Sets the X position in pixels of the start of the Annotation string.
setDisplayAnnotationY(int)-Method in class com.topaz.SigPlus
  Sets the Y position in pixels of the start of the Annotation string.
setDisplayjustifyMode(int)-Method in class com.topaz.SigPlus
  Sets the justification mode for how the signature is going to be sized and positioned in the box.
setDisplayJustifyX(int)-Method in class com.topaz.SigPlus
  Sets justification X coordinate in Logical Tablet Coordinates.
setDisplayJustifyY(int)-Method in class com.topaz.SigPlus
  Sets justification Y coordinate in Logical TAblet Coordinates.
setDisplayPenWidth(int)-Method in class com.topaz.SigPlus
  Sets pen width for displayed signature in pixels.
setDisplayRotation(int)-Method in class com.topaz.SigPlus
  Sets mode allowing signature rotation after capture.
setDisplayTimeStamp(boolean)-Method in class com.topaz.SigPlus
  Sets the bean to display the Time Stamp
setDisplayTimeStampSize(int)-Method in class com.topaz.SigPlus
  Sets the Y size in pixels of the Time Stamp.
setDisplayTimeStampX(int)-Method in class com.topaz.SigPlus
  Sets the X position in pixels of the start of the Time Stamp in the signature box.
setDisplayTimeStampY(int)-Method in class com.topaz.SigPlus
  Sets the Y position in pixels of the start of the Time Stamp in the signature box.
setDisplayTransparentMode(int)-Method in class com.topaz.SigPlus
  Sets whether the signature is displayed on a transparent background or not.
setEncryptionMode(int)-Method in class com.topaz.SigPlus
  Sets the encryption mode used for capturing signatures
setImageAnnotation(boolean)-Method in class com.topaz.SigPlus
  Sets whether or not the Annotation is being displayed as it apllies to a Java buffered image.
setImageAnnotationSize(int)-Method in class com.topaz.SigPlus
  Sets the size in pixels of the Annotation as it applies to a Java buffered image.
setImageAnnotationX(int)-Method in class com.topaz.SigPlus
  Sets the X position in pixels of the start of the Annotation as it applies to a Java buffered image.
setImageAnnotationY(int)-Method in class com.topaz.SigPlus
  Sets the Y position in pixels of the start of the Annotation as it applies to a Java buffered image.
setImageJustifyMode(int)-Method in class com.topaz.SigPlus
  Sets the justification mode for how the signature is diplayed as it applies to a Java buffered image.
setImageJustifyX(int)-Method in class com.topaz.SigPlus
  Sets justify X buffer in pixels as it applies to a Java buffered image.
setImageJustifyY(int)-Method in class com.topaz.SigPlus
  Sets justify Y buffer in pixels as it applies to a Java buffered image.
setImagePenWidth(int)-Method in class com.topaz.SigPlus
  Sets pen width for the signature as it applies to a Java buffered image.
setImageRotation(int)-Method in class com.topaz.SigPlus
  Sets the mode allowing for signature rotation after capture as it applies to a Java buffered image.
setImageTImeStamp(boolean)-Method in class com.topaz.SigPlus
  Sets the bean to display the Time Stamp as it applies to a Java buffered image.
setImageTimeStampSize(int)-Method in class com.topaz.SigPlus
  Sets the size in pixels of the Time Stamp as it applies to a Java buffered image.
setImageTimeStampX(int)-Method in class com.topaz.SigPlus
  Sets the X postition in pixels of the start of the Time Stamp as it applies to a Java buffered image.
setImageTimeStampY(int)-Method in class com.topaz.SigPlus
  Sets the Y position in pixels of the start of the Time Stamp as it applies to a Java buffered image.
setImageTransparentMode(boolean)-Method in class com.topaz.SigPlus
  Sets whether or not the signature is displayed on a transparent background as it applies to a Java buffered image.
setImageXSize(int)-Method in class com.topaz.SigPlus
  Sets the number of X pixels in the Java bufferd image.
setImageYSize(int)-Method in class com.topaz.SigPlus
  Sets the number of X pixels in the Java buffered image.
setLCDTabletMap(int, int, int, int, int, int)-Method in class com.topaz.SigPlus
  Overrides the default LCD parameters at run time.
setLCDCaptureMode(int)-Method in class com.topaz.SigPlus
  Sets the current LCD mode for the tablet.
setSaveSigInfo(boolean)-Method in class com.topaz.SigPlus
  Enables/Disables the saving of Time Stamp and Annotate Data in the signature.
setSigCompressionMode(int)-Method in class com.topaz.SigPlus
  Sets the current compression mode for signatures.
setSigString(string)-Method in class com.topaz.SigPlus
  Sets the signature string into the bean.
setTabletBaudRate(int)-Method in class com.topaz.SigPlus
  Sets the baud rate for the tablet.
setTabletClippingMode(boolean)-Method in class com.topaz.SigPlus
  Sets mode where signature points outside the set display area are not reported.
setTabletComPort(string)-Method in class com.topaz.SigPlus
  Sets the COM port to use.
setTabletFilterPoints(int)-Method in class com.topaz.SigPlus
  Sets the Tablet Filter Points.
setTabletFormat(int)-Method in class com.topaz.SigPlus
  Sets the tablet format.
setTabletInvisible(boolean)-Method in class com.topaz.SigPlus
  Sets SigPlus to run windowless.
setTabletLCDType(int)-Method in class com.topaz.SigPlus
  Sets the LCD type of the signature tablet.
setTabletLCDXSize(int)-Method in class com.topaz.SigPlus
  Sets the LCD tablet width in pixels.
setTabletXStart(int)-Method in class com.topaz.SigPlus
  Sets X pos in Logical Tablet Coordinates of left most pixel.
setTabletXStop(int)-Method in class com.topaz.SigPlus
  Sets the X pos in Logical Tablet Coordinates of right most pixel.
setTabletLCDYSize(int)-Method in class com.topaz.SigPlus
  Sets LCD tablet height in pixels.
setTabletLCDYStart(int)-Method in class com.topaz.SigPlus
  Sets Y pos in Logical Tablet Coordinates of top most pixel.
setTabletLCDYStop(int)-Method in class com.topaz.SigPlus
  Sets Y pos in Logical Tablet Coordinates of bottom most pixel.
setTabletModel(string)-Method in class com.topaz.SigPlus
  Sets the model for the signature tablet.
setTabletResolution(int)-Method in class com.topaz.SigPlus
  Sets tablet hardware resolution.
setTabletRotation(int)-Method in class com.topaz.SigPlus
  Sets the orientation for the display of tablet data.
setTabletState(int)-Method in class com.topaz.SigPlus
  Opens port to enable signature capture.
setTabletTimingAdvance(int)-Method in class com.topaz.SigPlus
  Sets the Tablet Timing Advance.
setTabletXStart(int)-Method in class com.topaz.SigPlus
  Sets the X pos of the top left corner of the signature box in Logical Tablet Coordinates.
setTabletXStop(int)-Method in class com.topaz.SigPlus
  Sets the X pos of the bottom right corner of the signature box in Logical Tablet Coordinates.
setTabletYStart(int)-Method in class com.topaz.SigPlus
  Sets the Y pos of the top left corner of the signature box in Logical Tablet Coordinates.
setTabletYStop(int)-Method in class com.topaz.SigPlus
  Sets the Y pos of the bottom right corner of the signature box in Logical Tablet Coordinates.
setTimeStamp(int)-Method in class com.topaz.SigPlus
  Sets the Time Stamp for the signature.
SigDataEventHandler-Interface com.topaz.SigPlus.SigDataEventHandler
  Interface for handling events from the SigPlus Java bean
sigImage()-Method in class com.topaz.SigPlus
  Returns a Java buffered image of the current signature using the image properties.
sigobj.AddSigPlusListener (new SigPlusListener)-Constructor in public interface SigEventDataHandler
  Listener for events that occur to the signature object within SigPlus
SigPlus-Class com.topaz.SigPlus
  Provides all the functionality required for customized capture and encryption of electronic handwritten biometric signatures.
SigPlus()-Constructor for class com.topaz.SigPlus
  Default Constructor

A C E G H I K L N S

Overview | Package | Class | Tree | Deprecated | Index | Help
| Topaz Systems, Inc. SigPlus v2.41
PREV NEXT | FRAMES NO FRAMES

Copyright © 2004 Topaz Systems, Inc. All rights reserved. Use is subject to license terms