To review the SigPlus javadocs, please open the sigplusjava_documentation folder, and double-click the api.html document.

The TopazAuto.inf and TopazUsb.sys files are for use with Topaz tablet models ending in "-USB". They are not necessary for use with tablet models ending in "-B" or "-HSB".

For all apps, the SigPlus2_xx.jar and the comm.jar (varies from one operating system to another) must be added to the classpath. 

For Windows apps, make sure the win32com.dll resides in the target machine's sys32 folder. Also, when using HSB/USB pads, copy the SigUsb.dll file to the target machine's sys32 folder, and also the location of the app itself.

For using the "HSB" pads under Linux, please refer to the SigPlusLinuxHSB.zip file, which contains a demo and dependencies.